Sensor Interfacing

Telemetry:

Temperature 0X10

Pressure 0X20

Humidity 0X30

State:

BME688\_Current\_Readings 0X10

Alarm:

Temperature Threshold 0X10

Pressure Threshold 0X20

Humidity Threshold 0X30